|  |  |
| --- | --- |
| Brand | Auto*Test* Products |
| Product Category | Diagnostics |
| Product Sub-Category | Passenger Vehicles |
| Main Page Heading | Auto*Light*®Window Tint Meter |
| Product Name | Auto*Light*®Plus |
| Primary Model | Auto*Light*® |
| Product Description | Auto*Light*® Plus is a Window Tint Meter that measures the level of light transmitted through a tinted window to determine its safety level.The Auto*Light*® Plus version allows results to be downloaded to a PC through a Bluetooth connection. This means that results can be collected, analysed and printed at the user’s convenience.**Features** * Easy to operate by aligning two reader tubes
* Simple one button operation
* Can be used for side windows or windscreens
* Calculates the percentage of light transmitted through windows
* Lightweight (350g)
* Compact (190mm x 60mm)
* Automatic start function
* Australian Made
* PC download capability through Bluetooth connection
* Stores last 20 tests to memory
* Compliant with ISO 3538:1997
* Optional Magnetic upgrade

**Upgrade to Auto*Light***® **MAGNETIC – Additional Features*** Magnetic for hands free operation
* Easy and accurate to operate by aligning two reader tubes, positioned with magnets

**Models Available*** Auto*Light*®
* Auto*Light*® Plus
* Auto*Light*® MAGNETIC

**Why Auto*Light*?**Window tinting can diminish driver vision through vehicle windows. This compromises the safety of the driver and their passengers. Safety is jeopardised when approaching vehicles with dark, nonregulatory approved window tinting. The internal space of the vehicle and its passenger’s movements are not clearly visible.**What is Auto*Light*?**Auto*Light*® is a portable Light Transmission Meter. The meter measures the level of light transmitted through a tinted window to determine its safety level. It is a lightweight, accurate and easy to operate tool for law enforcement officers. Some local regulations also require testing of tinted glass to ensure conformance during vehicle safety inspections. The Auto*Light*® meter provides inspectors with accurate readings that would otherwise be impossible by simple visual inspection.**Upgrade to Auto*Light***® **MAGNETIC** Roadworthy legislation has changed in some states. You are now required to take a photo of each window tint test result. Auto*Light*® MAGNETIC has magnets so you can test hands free! Making it possible for a single operator to take a photo of the results without dropping the Auto*Light*®. Magnets also make it faster for you to get accurate results as the testers line up perfectly every time. |
| Warranty  | 1 Year Parts & Labour Warranty |
| Optional Accessories | Auto*Light*® Plus is compatible with remote Auto*Test*® Bluetooth Printer |
| Specification Table | **Monitoring** • Compliant with ISO 3538:1997 • Spectral sensitivity conforming to photopic curve V (λ) of relative illuminous efficiency of the CIE 1931 standard observer for photopic vision **Output** • 2856ºK ± 50ºK, conforming to CIE illuminate A • Lamp voltage stabilisted within ±0.1% • Display: LED readout 0 - 100%, linear from 20 - 100%, ±3% **Power Source** • 2 x MN 1604 batteries (9 volt) |
| Image / Logo File Size | 300 – 400 kb  |
| Image / Logo Size | 1920px wide |
| Image / Logo Type | .jpeg or .png |
| Spec. Sheet Attachment | PDF file |
| Brochure Attachment | PDF file |