|  |  |
| --- | --- |
| Brand | Auto*Test* Products |
| Product Category | Diagnostics |
| Product Sub-Category | Diagnostic & Service Tool |
| Main Page Heading | Auto*Test*®Ultimate Roadworthy Kit |
| Product Name | Auto*Test*®Ultimate Roadworthy Kit |
| Primary Model | Auto*Test*®Ultimate Roadworthy Kit |
| Product Description | **THE ULTIMATE ROADWORTHY KIT**  A MUST HAVE FOR EVERY GARAGE FOR FAST & ACCURATE ROADWORTHY RESULTS.  Combines the Auto*Test* Workshop*Pro*® 10 brake meter tablet and Auto*Light*® MAGNETIC window tint meter with a Auto*Test*® Headlight Align headlight aimer to create the ultimate roadworthy kit.  This kit meets roadworthy requirements in WA, QLD, VIC, TAS, SA, NT & ACT\*.  *\*For ACT the Pedal Effort Sensor is an additional requirement to be compliant.*  The **Auto*Test* WorkshopPro® 10 tablet** is both a self-contained brake testing tool and an advanced workshop maintenance tool. Designed to test service and emergency brakes in passenger cars, trains, buses, farming and airport vehicles.  Send roadworthy photos and data directly to your state’s roadworthy authority, through their app. Download their app directly to the Workshop Pro 10.   * Workshop maintenance logging * Compliant with roadworthy regulations around Australia * Compliant with AS2958 Australian Standard * Compliant with SANS 1589 brake testing * Compliant with SANS 10047 brake testing * Compliant with ECE R13 – Rule 13 * Compliant with Federal Regulation FMVSS 135 and FMVSS 571 – USA * Compliant with Transport Canada – CMVSS 135 * Calibration that is internationally traceable through NATA (accreditation #20559) * Accident investigations * Brake system fault-finding   Compliant in Australia with roadworthy regulations in WA, QLD, VIC, TAS, SA, NT & ACT.\*  For ACT the Pedal Effort Sensor is an additional requirement to be compliant.  **Auto*Light*®** ***MAGNETIC*** is a Light Transmission Meter that measures the level of light transmitted through a tinted window to determine its safety level.  Our new Auto*Light*® MAGNETIC has magnets so you can test hands free! Making it possible for a single operator to take a photo of the results without dropping the Auto*Light*®. This is the fastest tint tester on the market, which gives accurate results with a single button operation.  Victorian legislation has changed for window tint testing. You are now required to take a photo of each window test result. As quoted by VicRoads regulations, dated 2012, “licensed vehicle testers must take and store digital photographs of the vehicles being inspected during a roadworthiness test.” Check the regulations in your area to see how it effects your testing requirements.   * Easy to operate by aligning two reader tubes * Hands-free testing * Single button operation * Compliant with roadworthy regulations * Compliant with ISO 3538:1997 * Lightweight (450g) * +/- 3% Accuracy   **Auto*Test*® Headlight Align** is a professional quality beam aligner suitable for all kinds of headlamps (high, low, fog including XENON and LED lamps). It is supplied with assembly, operation and calibration manuals and declaration of conformity.   * Robust anti-tip base fitted with large castors for easy manoeuvring * Laser pointers for easy positioning of the unit * Digital lux meter and wide measuring window * Manual optic alignment visor for easy parallel alignment * Easy-to-use height adjustment lock mechanism * Measuring distance: 500cm * Power consumption: <0.5W * Net Weight: 26kg   **Tests all classes of vehicles** |
| Warranty | 1 Year Parts & Labour Warranty |
| Optional Accessories | Upgrade to include the data management software for the Auto*Light* onto the Workshop Pro 10, for full integration and printing. |
| Specification Table | **Tests all classes of vehicles**  See each product page - Auto*Test* WorkshopPro® 10, Auto*Light*® MAGNETIC Light Transmission Meter and Auto*Tes*t® Headlight Align. |