|  |  |
| --- | --- |
| Brand | Auto*Test* Products |
| Product Category | Diagnostics |
| Product Sub-Category | Diagnostic & Service Tool |
| Main Page Heading | Auto*Test*®Brake Fluid Tester |
| Product Name | Auto*Test*®Brake Fluid Tester |
| Primary Model | Auto*Test*®Brake Fluid Tester |
| Product Description | The Auto*Test*®Brake Fluid Tester efficiently and accurately measures the moisture content in vehicle brake fluid.  **Features**   * Australian Made * User friendly * Accurate results shown in less than one minute * Suitable for use on new brake fluids and racing fluid * Helps prevent vapour lock and corrosion of engine parts * Increase brake servicing revenue * Suitable for use on new brake fluid and racing fluids * Measures boiling point, not conductivity (measuring boiling point is more accurate and repeatable.)   Brake fluid is designed to have a high boiling point to withstand the high temperatures generated by friction in the vehicle brake system. Unfortunately brake fluid readily absorbs moisture from air that transfers through the flexible rubber hoses. Moisture reduces its boiling point leading to possible brake failure.  Overseas studies have highlighted that over 50% of vehicles on the road today may have fluid that is too old to be within safety standards. Just like oil, brake fluid wears out and then it is simply not as reliable as fresh new brake fluid. In addition, moisture contaminated brake fluid can corrode internal parts within the braking system.  The Auto*Test* Brake Fluid Tester measures the moisture content in vehicle brake fluid. It provides accurate results in less than one minute that allows users to identify vehicles that require a brake fluid change. Consequently, it increases sales of brake fluid and brake fluid flushes.  The Brake Fluid Tester also increases the value of quick lube inspections, seasonal brake checks and routine servicing. Enhance your reputation for customer care and protect your clients by providing a brake fluid safety check. |
| Warranty | 1 Year Parts & Labour Warranty |
| Optional Accessories |  |
| Specification Table | **Technical Features**  • Operates off 12-volt supply - vehicles own battery  • LCD display  • Product dimensions: 2250mm (h) x 1000mm (w) x 806mm (d)  • 12 months warranty  • Internet support hotline  • Comprehensive after-sales service and assistance |